**PERRY COUNTY**

**INDIANA**

REGULAR PROPOSAL

CONTRACT AND BOND

FOR

**BITUMINOUS SURFACING**

**OF**

**BRUSHY FORK ROAD FROM TELL CITY LIMITS FOR 3.55 MILES TO ACORN ROAD AND CONTINUING 2.1 MILES ENDING AT STATE ROAD 145**

**PERRY COUNTY, INDIANA**

Bid Opening Date

April 1, 2024

Submitted By...

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Company Name

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Street and Number

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

City or Town State Zip Code

Specifications Prepared By

Perry County Highway Department

An Equal Opportunity Employer

**TABLE OF CONTENTS**

PERRY COUNTY, INDIANA

PROJECT: BRUSHY FORK ROAD FROM TELL CITY LIMITS FOR 3.55 MILES TO ACORN ROAD AND CONTINUING 2.1 MILES ENDING AT STATE ROAD 145

NOTE: It is each bidder’s responsibility to examine his proposal to determine that every sheet set out in the Table of Contents is attached and legible.

Table of Contents 2

Description of Work 3

Bid Form 4

Instructions to Bidders 5-6

Bid Bond 7

Special Provisions 8-14

Appendix 15

Agreement to Hold Harmless

Notice to Bidders

Form No. 96 – Contractors Bid for Public Works

Plan and Detail Sheet

Asphalt Temperature Form**GENERAL DESCRIPTION OF WORK**

All contract roads will include 18” wide stone shoulders and stone added to driveway approach for smooth transition, in accordance with the attached specifications. Milling required at bridges, paving limits and at asphalt/concrete driveways.

**BRUSHY FORK ROAD FROM TELL CITY LIMITS FOR 3.55 MILES TO ACORN ROAD CONTINUING 2.1 MILES ENDING AT STATE ROAD 145**

* Length 5.65 miles by 18’- 19’ wide
* Mobilization
* One lay of 1.5” HMA Type B Intermediate12.5 MM
* HMA Type B, Wedge and Level
* Asphalt for Tack Coat
* Limestone/shoulder stone #73 stone 18” wide compacted
* Millings with skid steer @ pavement tie-ins
* Maintenance of Traffic

**ITEMIZED BID FORM**

**SUBMITTED BY \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ DATE \_\_\_\_\_\_\_\_\_\_\_**

**BITUMINOUS SURFACING PROJECT**

**BRUSHY FORK ROADFROM TELL CITY LIMITS FOR 3.55 MILES TO ACORN ROAD AND CONTIMUING 2.1 MILES ENDING AT SR 145**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **DESCRIPTION** | **UNIT** | **QTY** | **UNIT PRICE** | **TOTAL** |
| Mobilization | LS | 1 |  |  |
| 1.75” HMA Type B, Surface 12.5 MM | TON | 6740.00 |  |  |
| HMA Type B,, Wedge and Level | TON | 825.00 |  |  |
| Asphalt for Tack Coat | TON | 21.00 |  |  |
| Compacted 73’s for Shoulder Stone | TON | 750.00 |  |  |
| Milling Tie-ins | SYD | 719.00 |  |  |
| Maintenance of Traffic | LS | 1 |  |  |

**INSTRUCTIONS TO BIDDERS**

**1. CONTRACT DOCUMENTS**

This entire bound set of documents shall serve as the "contract" for this project. The bid documents will consist of the following:

a.) Bid Form - fill-in the unit price, the extended amounts, and the TOTAL amount,

b.) State Form No. 96 - CONTRACTORS BID FOR PUBLIC WORKS(**NOTE** requirements of Sections II & III on SF96)

c.) Bid Bond.

After completing said forms the bidder shall place the contract documents in a sealed envelope which shall be clearly labeled as follows;

BID FOR BITUMINOUS SURFACING OF

BRUSHY FORK ROAD FROM TELL CITY LIMITS FOR 3.55 MILES TO ACORN AND ONTINUING 2.1 MILES ENDING AT SR 145

IN PERRY COUNTY, INDIANA

TO BE OPENED APRIL. 01, 2024

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_(Name of Bidder)

**2. BID DEPOSIT**

All sealed bids shall be received on or before 4:00 p.m. local time on Mar. 28, 2024 at the:

Perry County Auditor's Office

Perry County Courthouse

2219 Payne St.

Tell City, Indiana 47586

**3. BID OPENING**

1. All sealed bids received on or before 4:00 p.m. local time on Mar. 28, 2024 will be opened at 9:00 a.m. local time on Apr. 01, 2024 at the Perry County Commissioner's Meeting in the:

County Commissioner's Room

Perry County Courthouse

2219 Payne St.

Tell City, Indiana 47586

**4. AWARD**

The contract may be awarded at the Perry County Commissioners meeting on Apr. 01, 2024. The County Commissioners will execute State Form No. 96 at the time of award. All bids shall be subject to all requirements of the Contract Documents and these INSTRUCTION TO BIDDERS. All bids must be regular in every respect and no interlineations, excisions or special conditions shall be made or included in the Bid Form by the Bidders.

The Perry County Commissioners have the right to accept or reject any and all bids, and to award the contract for that bid which is most advantageous to Perry County.

No bidder may withdraw his proposal for a period of sixty (60) days after the date of opening thereof.

**5. INSURANCE CERTIFICATION & PAYMENT BOND**

The successful bidder shall deliver all properly executed insurance certifications and payment bond forms to the Perry County Auditor no less than one week after being awarded the contract. The failure of the bidder to deliver said insurance and bond documents within one week or within such extended period as the Perry County Commissioners may grant shall constitute a default and the Perry County Commissioners may award the contract to another bidder.

**6. NOTICE TO PROCEED**

The issuance of the notice to proceed for this project shall be issued within a reasonable time period. Paving operations shall begin within one month of the issuance of notice to proceed. subsequent to the issuance of the notice to proceed, the successful bidder must give the Perry County Highway Department no less than 3 work days notice prior to his beginning construction.

**7. CONTRACT COMPLETION**

The successful bidder will have 60 calendar days to complete the work as specified in this contract from the issuing date of the notice to proceed to the date of official acceptance of the work by the County of Perry.

**8. INTERPRETATIONS AND ADDENDA**

All questions about these contract documents should be made in writing to the County Highway Department so that they may become addenda to said contract documents. It shall be the responsibility of the bidder to inquire about any addenda to the contract documents prior to depositing the bid with the County Auditor. THE PERRY COUNTY COMMISSION RESERVES THE RIGHT TO DELETE ITEMS AND/OR CHANGE THEIR QUANTITIES AT ANY TIME PRIOR TO BID-OPENING BY MEANS OF WRITTEN ADDENDA.

**9. INSPECTION OF SITE**

Each bidder should visit the site of the proposed work and fully acquaint himself with the existing conditions there relating to the proposed improvement and should inform himself as to the facilities involved, the difficulties and the restrictions attending the performance of the Contract. The bidder shall thoroughly examine and familiarize himself with the Technical Specifications and all the other Contract Documents. The contractor by the execution of the Contract shall in no way be relieved of any obligation under it due to his failure to receive or examine any form or legal instrument or to visit the site and acquaint himself with the existing conditions.

**BID BOND**

PROJECT: Bituminous Surfacing Project on BRUSHY FORK ROAD FROM TELL CITY LIMITS FOR 3.55 MILES TO ACORN ROAD AND CONTINUING 2.1 NILES ENDING AT SR 145

KNOW ALL MEN BY THESE PRESENTS THAT \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_as principal,

and \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_as surety, are firmly bond unto the County of Perry, Indiana in the sum of

$1,000.00 of the principal’s bid, if after acceptance (receipt of the proposal by the County of Perry from the bidder) of the principal’s bid by the County of Perry said principal fails to enter into this contract for any reason whatsoever, and/or if for any reason said principal, after said bid has been so accepted by the County of Perry, fails to enter upon the performance of the obligation as set forth in said bid, we bind ourselves jointly and severally, and our joint and several heirs executors, administrators and assigns, firmly by these presents, this \_\_\_\_\_\_\_\_\_\_ day of \_\_\_\_\_\_\_\_\_\_\_, 2024.

The conditions of the above obligations shall be binding upon the principal and surety from the time said bid is filed with the County of Perry, Indiana until the regular Proposal and Contract Bond attached hereto shall be operative by the terms thereof.

IN WITNESS WHEREOF, we hereunto set our hands and seals this \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ day of \_\_\_\_\_\_\_\_\_\_\_, 2024.

Name\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

By \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ By \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature Title Signature Title

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Printed or Typed Printed or Typed

Surety Principal

State of Indiana, County of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, SS:

Personally appears before me \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ as principal and \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_as surety and each acknowledged the execution of the above Bid Bond this day of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, 2024.

Witness my hand and notarial seal the said last named date:

My Commission Expires: By\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Signature) (Notary Public)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

County of Residence (Printed or Typed)

**SPECIAL PROVISIONS**

BITUMINOUS SURFACING PROJECT ON Brushy Fork Road from Tell City Limits for 3.55 Miles to Acorn Road and continuing 2.1 Miles ending at SR 145

PERRY COUNTY, INDIANA

**SP 1. County Highway Superintendent**

Wherever the phrase "County Highway Superintendent" or "Highway Superintendent" or "Superintendent" appears in these special provisions it shall be understood that the phrase "or his/her designated field representative" is to be inserted immediately following.

**SP 2. Standard Specifications**

The Indiana Department of Transportation Standard Specifications dated 2012 and all related Supplemental Specifications, shall apply to this contract. Those Special Provisions, contained herein shall govern over the Standard Specifications and Supplemental Specifications should a conflict arise.

Construction signage shall be in accordance with the Indiana Manual on Uniform Traffic Control Devices (MUTCD). The contractor is responsible for all construction signage.

**SP 3. Payment Bond**

The contractor shall execute a payment bond to the appropriate political subdivision or agency, approved by and for the benefit of the political subdivision or agency, in an amount equal to the contract price. The payment bond is binding on the contractor, the subcontractor, and their successors and signs for the payment of all indebtedness to a person for labor and service performed, material furnished, or services rendered. The payment bond must state that it is for the benefit of the subcontractors, laborers, material suppliers, and those performing services.

A.) The payment bond shall be deposited with the board. The payment bond must specify that:

1.) A modification, omission, or addition to the terms and conditions of the public work, contract plans, specifications, drawings, or profiles;

2.) A defect in the public work contract; or

3.) A defect in the proceedings preliminary to the letting and awarding of the public work contract; does not discharge the surety. The surety of the payment bond may not be released until one (1) year after the board's final settlement with the contractor.

B.) A person to whom money is due for labor performed, material furnished, or services provided shall, within sixty (60) days after the completion of the labor or service, or within sixty (60) days after the last item of material has been furnished, file with the board signed duplicate statements of the amount due. The board shall forward to the surety of the payment bond one (1) of the signed duplicate statements. However, failure of the board to forward a signed duplicate statement does not affect the rights of a person to whom money is due. In addition, a failure to forward the statement does not operate as a defense for the surety.

C.) An action may not be brought against the surety until thirty (30) days after the filing of the signed duplicate statements with the board. If the indebtedness is not paid in full at the end of that thirty (30) day period the person may bring an action in court. The court action must be brought with sixty (60) days after the date of the final completion and acceptance of the public work.

**SP 4. Payment - Progress Estimates**

A.) The basis-of-pay for all items in the contract will be on a unit price basis per Indiana Department of Transportation (INDOT) procedures. The contractor will supply the County Highway Department with a copy of all material bills-of-lading, weight tickets, etc. on a weekly basis, and in a manner that is worked out with said Superintendent before work begins. The contractor will also supply the Superintendent a monthly progress estimate of work complete, in place, and approved by said Superintendent, filled out on blank bid forms, which may be obtained from the County Highway Department. Payment to the contractor will be made from said monthly estimates.

The contractor, if requested, shall be prepared to provide notarized material certificates for all materials furnished by him on this project. The Superintendent reserves the right to sample and test all material furnished on this project.

B.) Final payment - When the work has been completed in accordance with the terms of this contract and accepted by Perry County in writing a final estimate may be submitted to the County by the contractor. Final payment on that part of a contract or the amounts that are not in dispute shall be made within 120 days of final acceptance and completion of this contract.

**SP 5. Public Utilities**

The contractor shall make all necessary contacts and arrangements and work closely with all utilities having facilities within the project areas.

**SP 6. Responsibility for Damage Claims**

The Contractor shall save and hold harmless the Owner and the Superintendent and their officers, agents, and employees from and against all suits or claims that may be based upon alleged injury to any person or property that may occur, or may be alleged to have occurred in the course of the performance of the contract by the Contractor, whether such claims shall be made by an employee of the Contractor or by a third person, and whether or not it shall be claimed that the alleged injury was caused by a negligent act or omission of the Contractor; and The Contractor shall, at his own cost and expense, pay all charges of attorneys and all costs and other expense arising therefrom or incurred in connection therewith; and if any judgment shall be rendered against the Owner, the Superintendent, or any officer, agent, or employee of any thereof; the Contractor shall, at his own cost and expense, satisfy and discharge same.

**SP 7. Insurance**

The successful bidder (Contractor) will be required to furnish to the Owner prior to receiving the executed contract evidence that he has complied with all items of insurance listed hereinafter.

The Contractor shall carry in full force and effect during the period of contractual operations, insurance necessary to comply with the requirements of the Indiana Workmen's Compensation Act of the State of Indiana. Also, the Contractor shall carry in full force and effect during the period of contractual operations Occupational Diseases Insurance as set out in the Indiana Workmen's Occupational Diseases Act and shall file with the Owner certificates showing that said Workmen's Compensation (Industrial Board Form #19) and Occupational Diseases Insurance (Indiana Industrial Board Form #105) are in force during the period of contractual operations. The Contractor shall use his insurance carriers to furnish certificates for Compensation and Occupation Diseases Insurance to the Owner showing names of company’s expiration date or dates and policy number or numbers.

The Contractor shall take out and maintain during the life of the contract such Contractor's Comprehensive General Liability and Owner's and Contractors' Protective Liability Insurance as shall protect him and any subcontractor performing work covered by this contract from claims for damage or personal injury including accidental death as well as claims for property damage which may arise from operations under this contract whether such operations be by himself or by a subcontractor or by anyone directly or indirectly employed by either of them, and the minimum amounts of such insurance as set forth per Section 103.04 of the Standard Specifications. \*Furthermore, the Contractor shall use his insurance carriers to furnish certificates for such insurance showing Perry County, Indiana and Perry County, Indiana Board of Commissioners as additional insureds on such policies, together with names of companies expiration date or dates and policy number or numbers.\*

Insurance is required as a measure of protection and the Contractor's liability is not to be limited by the amount specified in the insurance policies.

If an expiration date on any of these policies occurs before the completion and acceptance of the project, an addenda certificate shall be furnished showing the new expiration date.

**SP 8. Incidental Construction / Maintenance of Traffic / Mobilization**

Where "Incidental Construction" has been indicated on the Plans in areas between new construction and existing pavement, any items necessary to provide a smooth transition between the new construction and existing surface shall be included in this work. Payment for this work shall be made at the Contract Unit Price of the various items necessary to complete this transitional work.

All costs associated with Maintenance of Traffic & Mobilization shall be included in the unit prices of items.

**SP 9. Noise Abatement & Working Time Restrictions**

The Contractor shall insure that all construction equipment is properly maintained and in proper working condition.

Work will only be allowed between sunrise and sunset as established by the U.S. Weather Bureau. Work will not be allowed on Saturdays, Sundays or Holidays, except that the Contractor may be allowed to work on the following holidays: Martin Luther King Day, President's Day, Good Friday, Primary Election Day, Columbus Day, Election Day and Veteran's Day. The Contractor must request permission to perform work on a holiday in writing from the County Highway Superintendent.

**SP 10. Bituminous Materials**

*General*

The Indiana Department of Transportation (INDOT) Standard Specifications 2012, Section 402, shall apply with the exceptions as noted herein. The current version of the INDOT Specifications, Recurring Special Provisions, and Supplemental Specifications are applicable.

Description:This work shall consist of one or more courses of HMA base, intermediate, surface mixtures or other miscellaneous HMA application in accordance with Indiana Test Method (ITM) 583. 402.02 shall not apply.

Design Mix Formula and Mixture Type:Contractor must submit a Design Mix Formula (DMF) to the Highway Superintendent for approval**. *ONLY HMA MIXES WILL BE ALLOWED.*** The design mix formula, prepared in accordance with 402.04, shall be based on the following table:

|  |  |  |  |
| --- | --- | --- | --- |
| ***Mixture Type*** | ***Type A*** | ***Type B*** | ***Type C*** |
| *Design ESAL* | *200,000* | *2,000,000* | *9,000,000* |
| *AADT* | *<4000* | *4000-30,000* | *>30,000* |
| *Surface* | *4.75, 9.5, 12.5 mm* | *4.75, 9.5, 12.5 mm* | *4.75, 9.5, 12.5 mm* |
| *Surface - PG Binder* | *64-22* | *64-22* | *70-22* |
| *Intermediate* | *9.5, 12.5,19.0, 25 mm* | *9.5, 12.5,19.0, 25 mm* | *9.5,12.5,19.0, 25 mm* |
| *Intermediate - PG Binder* | *64-22* | *64-22* | *64-22* |
| *Base* | *19, 25.0 mm* | *19, 25.0 mm* | *19, 25.0 mm* |
| *Base - PG Binder* | *64-22* | *64-22* | *64-22* |

Surface Aggregate Type:For Type C mixtures, surface aggregates shall meet the requirements for less than 10,000,000 ESAL in 904.03(d).

Acceptance of Mixtures:Acceptance shall be based on 402.09. The Type D Certification shall include the PG Binder Grade sent to the project.

draft

Temperature of Asphalt: Contractor is responsible for recording the temperature of the HMA, once per hour, and supplying the Superintendent with a daily report verifying temperature.

Minimum temperature Wedge & Level, Intermediate and Base HMA mixtures at the time it is placed in the paving machine shall be 290 degrees. Minimum temperature of Surface HMA mixtures at the time it is placed in the paving machine shall be 300 degrees. The Contractor will use the temperature recording forms supplied by Perry County. Random temperature checks will also be taken by the Perry County Superintendent or his/her field representative.

*Compaction*

It will be required to have two rollers on the HMA Surface lay and on full width paving.

*Tack Coat*

Shall be applied in such a manner as to offer the least inconvenience to traffic and to permit one-way traffic without pickup and tracking of bituminous material. If, after the application of the tack coat, it becomes necessary to open the section to traffic, cover aggregate shall be spread as directed by the Superintendent. The cover aggregate, if used shall be fine aggregate No. 23 or 24 and will not be paid for directly, but shall be included in the cost of other items.

*Pavement Patching*

A.) For failed Pavement - If the need should arise, and ONLY AT THE DIRECTION OF THE SUPERINTENDENT, to patch a section of the existing pavement that has “failed” the following shall apply:

The total depth requirement for patching flexible pavement, as described in the Standard Specification Section 304.04, is hereby amended to be SIX (6) inches. The material under the patch is expected to be in a compacted condition in accordance with said Specification 304.04.

B.) Payment - shall be paid for under HMA BASE, TYPE B 25.0mm FOR PATCHING.

C.) Special attention shall be paid to Standard Specification Section 105.12 (Load Restrictions) by the contractor.

*Bituminous Mixture for Approaches (Standard Specification Section 610)*

A.) Drive Approaches: The **18”** wide bituminous wedge for private drives described in Standard Specification Section 610.01 shall be required on this project. If an existing bituminous drive or concrete is encountered a smooth transition from new pavement to old pavement shall be constructed. Milling at the drive will be required.

Payment - the accepted quantities for said drive approaches shall be paid for at the contract unit price per ton for the mainline bituminous material.

B.) Public Road Approaches: Only those road approaches so detailed on the plans, shown on the Schedule of Approaches, or directed by the Superintendent shall be paved and paid for at the contract unit price per ton for the mainline bituminous material. Special attention should be paid to the plans as to the type of bituminous material that is to be used on a particular road approach. The length to be paved shall be as planned or as directed by the Superintendent.

C.) Mailbox Approaches – shall be resurfaced to cover existing pavement.

**SP 11. Maintaining Traffic**

Unless otherwise directed or permitted by the Superintendent, the Contractor shall arrange and prosecute the work specified for this contract in accordance with all applicable provisions of 104.04, 107, 801 and 923 of the 2012 Standard Specifications, the latest revised Standard of Detour Signs and Sign Design Details of the Indiana Department of Transportation Standards, the Indiana Manual on Uniform Traffic Control Devices, and as set out herein. Cost for Maintenance of Traffic shall be included in the price of bid items.

*Construction Under Traffic*

It is the intent of this contract that all work shall be done while the road is open to traffic and during the daylight hours. All Type "A" Construction Signs shall be furnished, erected, and maintained by the Contractor. The Contractor must request permission to close a road, in writing, from the County Highway Superintendent.

A.) All control devices including flagmen, shall be positioned so as to have a safe sight distance considering the approach speed for approaching traffic. The flagmen shall be equipped with portable two-way radios.

B.) All non-fixed signs are to be removed at the completion of the day's operation(s). All lanes will be open to normal traffic during the hours of darkness. If for any reason, a traffic lane must remain closed after dark, the Contractor will be required to maintain traffic on the remaining lane(s) in accordance with the latest revised Standard Sheets of the Standard Detour Signs of the Indiana Department of Transportation Standards. The Contractor will NOT be required to provide a night watchman to maintain the traffic control devices as described in INDOT Specification No. 107.12, on a 24-hour basis. The Contractor WILL, however, be required to inspect and maintain said traffic control devices, as described in INDOT Specification 107.12 no less than every eight (8) hours.

*Basis of Payment*

A.) It is the intent of this contract that maintenance of traffic is at the discretion of the contractor. Traffic shall be maintained in a manner which provides a safe environment for construction workers and the traveling public. See item SP6 of these specifications.

B.) All signs, flagmen, etc. that are needed to control traffic for construction under-traffic, should the need arise by the contractors choosing, shall be included in the price of the other bid items.

**SP 12. Pavement Traffic Markings**

Pavement markings are not part of this contract.

**SP 13. Signage**

The placement of all signs, construction or otherwise, shall be in accordance with the plans, but their final locations shall be approved by the County Highway Superintendent.

**SP 14. Heavy Truck Routes**

**EACH BIDDER IS REQUIRED TO CONTACT THE COUNTY ROAD SUPERINTENDENT PRIOR TO SUBMITTING BIDS TO DISCUSS AND DETERMINE HEAVY TRUCK ROUTES IN ORDER TO MINIMIZE DAMAGES TO EXISTING COUNTY ROADS.**

**SP 15. Nondiscrimination of Employees**

In the performance of this contract, the Contractor shall not discriminate against any worker because of race, religion, color, sex, national origin, or ancestry.

**SP 16. Payment of Minimum Wages**

The minimum wage paid to all labor shall be in accordance with all relevant Federal and Local Laws.

**SP 17. Safety; Accident Prevention**

In the performance of this contract, the contractor shall comply with all applicable Federal, State and local laws governing safety, health and sanitation. The contractor shall provide all safeguards, safety devices and protective equipment and take any other needed actions, on his own responsibility, or as either the County Highway Superintendent or his designated field representative may determine, reasonably necessary to protect the life and health of employees on the job and the safety of the public and to protect property in connection with the performance of the work covered by the contract.

**SP 18. Preparation of Road**

The Contractor shall be responsible for performing all work necessary to prepare the road and shoulders for completion of the work set forth in this contract unless otherwise noted. The Perry County Highway Department will mow and grade back the edges prior to paving, but the contractor will be responsible for brooming of roadway.

**APPENDIX**